*********************************************************** 
*                                                           
*  Axalto e-gate USB smart card drivers
*	  version 3.0.6.0
*
*  Installation Readme                                                           
*
************************************************************


************************************************************
*  CONTENTS OF THIS DOCUMENT
************************************************************
This document contains the following sections:

1.  Overview
2.  System Requirements
3.  Contents of the Distribution Package
4.  Windows Server 2003 Installation notes



************************************************************
* 1.  OVERVIEW
************************************************************
The installation program will install to the target system 
the Axalto e-gate USB smart card device drivers.

If a previous version of these drivers is already installed,
the installer will update these drivers to the current version.

The default installation directory is :
	<PROGRAM FILES>\Axalto\e-gate drivers 3.0.6.0

	 

************************************************************
* 3.  CONTENTS OF THE DISTRIBUTION PACKAGE
************************************************************
The e-gate USB smart card drivers installation package 
contains the following items:

    File(s)       
    -------
    Axalto-egate-drivers-v3.0.6.0.msi
    readme.txt (this file)



************************************************************
* 2.  SYSTEM REQUIREMENTS 
************************************************************
This software is intended for the following Operating systems :
	Windows 2000, Windows XP
	Windows Server 2003.

These drivers installation is done using the Microsoft Windows 
Installation service and can be executed in a silent mode.
For more information, see the Windows installer (msiexec) command
line options.

During the installation, a logging file named "egateinstall.log"
is created in the installation directory.



************************************************************
* 4.  WINDOWS SERVER 2003 INSTALLATION NOTES
************************************************************
On Windows Server 2003 and later versions, if the device setup class of a
driver package is not included in the Windows Logo Program, this package
cannot obtain a WHQL digital signature and the publisher is responsible for
digitally signing the driver using the Microsoft Authenticode technology. 

As the e-gate device driver setup class is not included in the Windows Logo
Program, when the driver is installed, the Axalto publisher certificate is
displayed and the user must accept to trust Axalto to continue the installation.

In order to avoid this process during a silent installation, the administrator
can add the publisher certificate to the trusted publisher certificate store,
before executing the setup program.

The Axalto publisher certificate can be provided as needed.
Contact the Axalto support services.

