Installation...

IMPORTANT - Do not connect the Smart Card Reader to your PC until software is installed and computer is restarted.

1.          Close down all running applications. 

2.          Unpack Pkey_driver.rar and start driver instalation.

3.          To restart your computer and finish installation, click finish.

4.          Connect Smart Card reader directly into USB port or with a hub. Wait for Windows to install your new hardware.

5.          Insert Smart Card. A green light should appear, indicating Smart Card Manager is correctly installed.


Have fun,
JAFWM Team
